Parts to be sent to Magnetic Shields

For alterations

|  |  |
| --- | --- |
| Item | Notes |
| 1 cylindrical tube 170 diameter 985mm height (Inner shield) | 3 holes enlarged as per drawings and heat treated |
| 1 half semi-circular end cap 612 mm diameter | 1 hole drilled as per drawings (location roughly marked on cap) and heat treated |
| 1 half semi-circular end cap 612 mm diameter | 1 hole drilled as per drawings (location roughly marked on cap) and heat treated |
| 1 half cylindrical tube 800mm height labelled “Bottom front” with attached band | 1 hole drilled as per drawings and heat treated |
| 1 half cylindrical tube 800mm height labelled “Bottom back” with attached band | 1 hole drilled as per drawings and heat treated |

For scrap

|  |  |
| --- | --- |
| Item | Notes |
| 1 half cylindrical tube 800mm height labelled “Top front” marked “Scrap” |  |
| 1 half cylindrical tube 800mm height labelled “Top back” marked “Scrap” |  |
| 4 Shield quarter sections 1420 mm height marked “Scrap” |  |